#!/bin/bash
#
REPO_PATH="$(/usr/bin/dirname $([ -L $0 ] && /bin/readlink -f $0 || echo $0))"
source "${REPO_PATH}/install.common"

check_if_installed

echo "Loading Loopback device"
modprobe snd-aloop || exit 1

LOOPBACK_CARD_ID=$(grep -F "[Loopback" < /proc/asound/cards | awk '{print $1}')
if [[ ! $(echo "$LOOPBACK_CARD_ID" | grep -E "^[0-9]$") ]]
then
	echo "Error: Could not determine Loopback card number"
	exit 1
fi

if [ -d "/etc/modprobe.d/" ]; then
	add_line "/etc/modprobe.d/droidcam.conf" "options snd-aloop index=$LOOPBACK_CARD_ID"
fi

if [ -d "/etc/modules-load.d" ]; then
	add_line "/etc/modules-load.d/droidcam.conf" "snd-aloop"
elif [ -e "/etc/modules" ]; then
	add_line "/etc/modules" "snd-aloop"
else
	echo "Warning: Unknown distro. Sound card may not load after a reboot."
fi

echo "Done"
echo "Use 'pacmd load-module module-alsa-source device=hw:Loopback,1,0' to load the card into PulseAudio while droidcam is running"